Share this page

# Configure Micro Focus Connect for SSL/TLS

This topic describes how to configure Micro Focus Connect to be accessible over SSL/TLS.

In this topic:

## Basic SSL/TLS

Micro Focus Connect is installed as a web application within an Apache Tomcat web server.

To set up basic SSL/TLS configuration:

1. Follow the steps as per the Apache Tomcat 9 documentation for SSL/TLS.

2. Restart Tomcat. The server now supports SSL via HTTPS.

The following is an example of a connector specification when you specify the keystorePass and keyPass parameters in clear text:

<Connector port="443" maxHttpHeaderSize="8192" maxThreads="100"

minSpareThreads="25" maxSpareThreads="75"

enableLookups="false" disableUploadTimeout="true"

acceptCount="100" scheme="https" secure="true"

SSLEnabled="true" clientAuth="false"

sslProtocol="TLS" keyAlias="tomcat"

keystoreFile="conf/.ssl/keystore.jks"

keystorePass="password"

keyPass="certpass"/>

For information on how to decrypt the keystorePass and keyPass parameters, see below.

Back to top

Next steps:

- Install SSL certificates
- Create a data source

https://admhelp.microfocus.comMicro Focus Connect8942
Tips to improve your search results... Micro Focus Connect Help CenterMF Connect Help4.0-4.4.3AllView Local Help CenterView Online Help CenterbackGo back in browser historyforwardGo forward in browser historyRemove search highlightsnext topicGo to next topicprevious topicGo to previous topicPrint the current topicVersion: