Share this page

# Network Sub-Path Time graph

This graph displays the delay from the source machine to each node along the path according to the elapsed load test scenario time. You can use the graph to determine the sub-path in which there was a delay, the length of the delay, and at what time the delay occurred.

The delays from the source machine to each of the nodes are measured concurrently, yet independently. It is therefore possible that the delay from the source machine to one of the nodes could be greater than the delay for the complete path between the source and destination machines.

Each sub-path is displayed as a separate line with a different color.

Axis | Description
--- | ---
X-axis | Elapsed time since the start of the run.
Y-axis | Network delay time.

Back to top

See also:

- Network delay monitoring
- Network Monitor graphs

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 25.1-25.3 All View Local Help Center View Online Help Center Version: