Share this page

# Average Bandwidth Utilization graph

This graph shows the average bandwidth utilized by a virtual user or a virtualized location from the maximal available bandwidth allocated for it during the last second, measured in percentages.

You cannot change the granularity of the x-axis to a value that is less than the web granularity you defined in the General tab of the Options dialog box.

For Analysis (not applicable to monitoring graphs):

To view information for a specific location:

1. Click within the graph.
2. Select Set Filter/ Sort By from the right-click menu to open the Graph Settings dialog box.
3. In the Filter condition section, select the Location Name row, and select the relevant location from the drop-down list.

Axis | Description
--- | ---
X-axis | Elapsed time since the start of the run.
Y-axis | The percentage of bandwidth utilization.

If you enabled Network Virtualization per load generator (and not per group), the graph shows the measurements per load generator, as shown in the Packet Loss graph.

Back to top

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 25.1-25.3 All View Local Help Center View Online Help Center Version: