Share this page

# Network Segment Delay graph

This graph shows the delay for each segment of the path according to the elapsed load test scenario time. You can use the graph to determine the segment in which there was a delay, the length of the delay, and the time at which the delay occurred.

Each segment is displayed as a separate line with a different color.

Item | Description
--- | ---
X-axis | Elapsed time since the start of the run.
Y-axis | Network delay time.
Note | The segment delays are measured approximately, and do not add up to the network path delay which is measured exactly. The delay for each segment of the path is estimated by calculating the delay from the source machine to one node and subtracting the delay from the source machine to another node. For example, the delay for segment B to C is calculated by measuring the delay from the source machine to point C, and subtracting the delay from the source machine to point B.

Back to top

See also:

- Network delay monitoring
- Network Monitor graphs

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 25.1-25.3 All View Local Help Center View Online Help Center Version: