Share this page

# Load Generator Configuration > Connection tab

This tab enables monitoring or running Vusers over a firewall. It also allows you to select a connection profile for communication between the load generator and the MI Listener or the Data Hub.

To access, click Controller toolbar > Load Generators button > Add > More .

Important:

- If the load generator is connected, you cannot change values in this tab. To disconnect a load generator, select it in the Load Generators dialog box and click Disconnect. The load generator status changes to Down, and you can change the settings.
- If the load generator is localhost, this tab is disabled.

User interface elements are described below:

UI Element | Description
--- | ---
Choose Network Profile | A drop-down list of network profiles defining the connection properties of the load generator. Each profile defines whether to connect using direct TCP connection, using MI Listener, or using the Data Hub. It also includes information to connect to the load generator using a proxy (if relevant). Click Browse to open the Network Profile Manager. For details, see Network Profile Manager dialog box.
Enable Monitoring over Firewall | Enables monitoring over firewall for this load generator.

Back to top

See also:

- Add load generators to a scenario
- Add New Load Generator/Load Generator Information dialog box
- Data Hub and Web Connector setup

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 25.1-25.3 All View Local Help Center View Online Help Center Version: