Share this page

# Average Throughput graph

This graph shows the average data traffic passing to or from the virtualized location (input and output traffic for both the server and client machines), measured in kilobytes per second (kBps). It helps you evaluate the amount of load Vusers generated, in terms of the number of server and client throughput. Use the legend below the graph to determine the line color for each metric. You cannot change the granularity of the x-axis to a value that is less than the web granularity you defined in the General tab of the Options dialog box.

For example, you can use this graph to identify the group for which the average server input throughput was the lowest. For more information, see Total Throughput graph.

If you enabled Network Virtualization per load generator (and not per group), the graph shows the measurements per load generator, as shown in the Packet Loss graph.

For Analysis (not applicable to monitoring graphs):

To view information for a specific location:

1. Click within the graph.
2. Select Set Filter/ Sort By from the right-click menu to open the Graph Settings dialog box.
3. In the Filter condition section, select the Location Name row, and select the relevant location from the drop-down list.

Axis | Description
--- | ---
X-axis | Elapsed time since the start of the run.
Y-axis | The rate of data passing to and from the virtual location, in bps for the following metrics per group or load generator: Input to the client machine Output from the client machine Input to the server machine Output from the server machine

Back to top

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 25.1-25.3 All View Local Help Center View Online Help Center Version: