Share this page

# Citrix measurements

The Citrix Server monitor provides you with information about the application deployment usage of the Citrix server during a load test scenario execution.

In this topic:

## Non-virtual counters

Measurement | Description
--- | ---
% Disk Time | The percentage of elapsed time that the selected disk drive services read or write requests.
% Processor Time | The percentage of time that the processor executes a non-Idle thread. This counter is a primary indicator of processor activity. It is calculated by measuring the time that the processor spends executing the thread of the Idle process in each sample interval, and subtracting that value from 100%. (Each processor has an Idle thread which consumes cycles when no other threads are ready to run.) It can be viewed as the percentage of the sample interval spent doing useful work. This counter displays the average percentage of busy time observed during the sample interval. It is calculated by monitoring the time the service was inactive, and then subtracting that value from 100%.
File data Operations/sec | The rate that the computer issues Read and Write operations to file system devices. It does not include File Control Operations.
Interrupts/sec | The average number of hardware interrupts the processor receives and services per second. It does not include DPCs, which are counted separately. This value is an indirect indicator of the activity of devices that generate interrupts, such as the system clock, the mouse, disk drivers, data communication lines, network interface cards and other peripheral devices. These devices normally interrupt the processor when they have completed a task or require attention. Normal thread execution is suspended during interrupts. Most system clocks interrupt the processor every 10 milliseconds, creating a background of interrupt activity. This counter displays the difference between the values observed in the last two samples, divided by the duration of the sample interval.
Output Session Line Speed | This value represents the line speed from server to client for a session in bps.
Input Session Line Speed | This value represents the line speed from client to server for a session in bps.
Page Faults/sec | A count of the Page Faults in the processor. A page fault occurs when a process refers to a virtual memory page that is not in its Working Set in main memory. A Page Fault does not cause the page to be fetched from disk if that page is on the standby list, and hence already in main memory, or if it is in use by another process with whom the page is shared.
Pages/sec | The number of pages read from the disk or written to the disk to resolve memory references to pages that were not in memory at the time of the reference. This is the sum of Pages Input/sec and Pages Output/sec. This counter includes paging traffic on behalf of the system Cache to access file data for applications. This value also includes the pages to/from non-cached mapped memory files. This is the primary counter to observe if you are concerned about excessive memory pressure (that is, thrashing), and the excessive paging that may result.
Pool Nonpaged Bytes | The number of bytes in the Nonpaged Pool, a system memory area where space is acquired by operating system components as they accomplish their appointed tasks. Nonpaged Pool pages cannot be paged out to the paging file, but instead remain in main memory as long as they are allocated.
Private Bytes | The current number of bytes this process has allocated that cannot be shared with other processes.
Processor Queue Length | The instantaneous length of the processor queue in units of threads. This counter is always 0 unless you are also monitoring a thread counter. All processors use a single queue in which threads wait for processor cycles. This length does not include the threads that are currently executing. A sustained processor queue length greater than two generally indicates processor congestion. This is an instantaneous count, not an average over the time interval.
Threads | The number of threads in the computer at the time of data collection. Notice that this is an instantaneous count, not an average over the time interval. A thread is the basic executable entity that can execute instructions in a processor.
Latency – Session Average | The average client latency over the life of a session.
Latency – Last Recorded | The last recorded latency measurement for this session.
Latency – Session Deviation | The difference between the minimum and maximum measured values for a session.
Input Session Bandwidth | The bandwidth (in bps) from client to server traffic for a session in bps.
Input Session Compression | The compression ratio for client to server traffic for a session.
Output Session Bandwidth | The bandwidth (in bps) from server to client traffic for a session.
Output Session Compression | The compression ratio for server to client traffic for a session.
Output Session Linespeed | The line speed (in bps) from server to client for a session.

Back to top

## Virtual channel counters

All the counters in the following table are measured in bytes per second (bps):

Measurement | Description
--- | ---
Input Audio Bandwidth | The bandwidth from client to server traffic on the audio mapping channel.
Input Clipboard Bandwidth | The bandwidth from client to server traffic on the clipboard mapping channel.
Input COM1 Bandwidth | The bandwidth from client to server traffic on the COM1 channel.
Input COM2 Bandwidth | The bandwidth from client to server traffic on the COM2 channel.
Input COM Bandwidth | The bandwidth from client to server traffic on the COM channel.
Input Control Channel Bandwidth | The bandwidth from client to server traffic on the ICA control channel.
Input Drive Bandwidth | The bandwidth from client to server traffic on the client drive mapping channel.
Input Font Data Bandwidth | The bandwidth from client to server traffic on the local text echo font and keyboard layout channel.
Input Licensing Bandwidth | The bandwidth from server to client traffic on the licensing channel.
Input LPT1 Bandwidth | The bandwidth from client to server traffic on the LPT1 channel.
Input LPT2 Bandwidth | The bandwidth from client to server traffic on the LPT2 channel.
Input Management Bandwidth | The bandwidth from client to server traffic on the client management channel.
Input PN Bandwidth | The bandwidth from client to server traffic on the Program Neighborhood channel.
Input Printer Bandwidth | The bandwidth from client to server traffic on the printer spooler channel.
Input Seamless Bandwidth | The bandwidth from client to server traffic on the Seamless channel.
Input Text Echo Bandwidth | The bandwidth from client to server traffic on the local text echo data channel.
Input Thinwire Bandwidth | The bandwidth from client to server traffic on the Thinwire (graphics) channel.
Input VideoFrame Bandwidth | The bandwidth from client to server traffic on the VideoFrame channel.
Output Audio Bandwidth | The bandwidth from server to client traffic on the audio mapping channel.
Output Clipboard Bandwidth | The bandwidth from server to client traffic on the clipboard mapping channel.
Output COM1 Bandwidth | The bandwidth from server to client traffic on the COM1 channel.
Output COM2 Bandwidth | The bandwidth from server to client traffic on the COM2 channel.
Output COM Bandwidth | The bandwidth from server to client traffic on the COM channel.
Output Control Channel Bandwidth | The bandwidth from server to client traffic on the ICA control channel.
Output Drive Bandwidth | The bandwidth from server to client traffic on the client drive channel.
Output Font Data Bandwidth | The bandwidth from server to client traffic on the local text echo font and keyboard layout channel.
Output Licensing Bandwidth | The bandwidth from server to client traffic on the licensing channel.
Output LPT1 Bandwidth | The bandwidth from server to client traffic on the LPT1 channel.
Output LPT2 Bandwidth | The bandwidth from server to client traffic on the LPT2 channel.
Output Management Bandwidth | The bandwidth from server to client traffic on the client management channel.
Output PN Bandwidth | The bandwidth from server to client traffic on the Program Neighborhood channel.
Output Printer Bandwidth | The bandwidth from server to client traffic on the printer spooler channel.
Output Seamless Bandwidth | The bandwidth from server to client traffic on the Seamless channel.
Output Text Echo Bandwidth | The bandwidth from server to client traffic on the local text echo data channel.
Output Thinwire Bandwidth | The bandwidth from server to client traffic on the Thinwire (graphics) channel.
Output VideoFrame Bandwidth | The bandwidth from server to client traffic on the VideoFrame channel.

Back to top

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 25.1-25.3 All View Local Help Center View Online Help Center Version: