Share this page

# IP Wizard

This wizard enables you to create and save new IP addresses on Windows machines.

Item | Description
--- | ---
To access | Search for IP Wizard in the Windows Start menu.
Important information | This wizard resides on each load generator. It enables you to create and save new IP addresses on Windows machines. The new addresses can be a range of addresses defined by the Internet Assignment Numbers Authority. They are for internal use only, and cannot connect to the Internet. This range of addresses is the default used by the IP Wizard. You must be logged in with administrator permissions to run the IP Wizard.
Relevant tasks | Add IP addresses to a load generator
See also | General tab

User interface elements for all wizard pages are described below:

Option | Description
--- | ---
Create new settings | Enables you to define new IP settings on the load generator.
Load previous settings from file | Enables you to use an existing file with IP address settings.
Restore Original Settings | Restores original settings.
<Web Server Address box> | If you have more than one network card, enables you to choose the card to use for IP addresses. This step enables the IP Wizard to check the server's routing table to see if it requires updating after new IP addresses are added to the load generator.
Add button | Opens the Add dialog box where you can add new IP addresses. The Add dialog box contains the following options: Private Address Spaces. Classes that represents the correct submask for the machine's IP addresses. From IP. Adds IP addresses starting with this number. Number to add. The number of IP addresses to add. Submask. IP addresses include two components, a netid and hostid. The submask determines where the netid portion of the address stops and where the hostid begins. Automatically add IP addresses. IP addresses are automatically detected and added based on network settings. Default setting: Not selected. Verify that new IP addresses are not already in use. Instructs the IP Wizard to check the new addresses. The IP Wizard adds only the addresses that are not already in use.
Remove button | Removes a selected IP address.
IP Address | The IP addresses on the load generator machine.
Subnet Mask | The submasks of the IP addresses on the load generator machine.
Number of IPs added | The number of IP addresses added to the load generator machine.
Finish button | Click Finish to exit the IP Wizard and add the addresses to the IP pool. The IP Wizard runs a netsh batch file to update the NT device drivers with the new addresses.
<Summary area> | Displays a summary of the operations performed by the IP Wizard. Take note of the location of the netsh batch file (.bat). This is used to update the routing table, if necessary. See Add IP addresses to a load generator.

Back to top

See also:

- Add IP addresses to a load generator
- Multiple IP addresses

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 25.1-25.3 All View Local Help Center View Online Help Center Version: