Share this page

# Network communications

When setting up your load testing network, you must plan the communications between Controller and other components.

To enable internal communications between Controller and other components, make sure that port 5976 is kept open on the Controller machine.

This section includes:

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 26.1-26.3 All View Local Help Center View Online Help Center Version: