Share this page

# Infrastructure Resources graph

The Infrastructure Resource monitor provides you with information about the performance of FTP, POP3, SMTP, IMAP, and DNS Vusers on the network client during load test scenario execution.

In this topic:

## Network Client graph

The Network Client graph displays network client data points for FTP, POP3, SMTP, IMAP, and DNS Vusers during a load test scenario run.

Axis | Description
--- | ---
X-axis | The elapsed time since the start of the run.
Y-axis | The resource value of the network client data points.

# Network Client measurements

Measurement | Description
--- | ---
Pings per sec | Number of pings per second.
Data transfer bytes per sec | Number of data bytes transferred per second.
Data receive bytes per sec | Number of data bytes received per second.
Connections per sec | Number of connections per second.
Accept connections per sec | Number of connections accepted per seconds.
SSL Connections per sec | Number of SSL connections per second.
SSL Data transfer bytes per sec | Number of SSL data bytes transferred per second.
SSL Data receive bytes per sec | Number of SSL data bytes received per second.
SSL Accept connections per sec | Number of SSL connections accepted per seconds.

## See also

- Infrastructure Resources monitoring

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 26.1-26.3 All View Local Help Center View Online Help Center Version: