Share this page

# Average Latency monitor graph

This graph shows the average recorded time required for a packet of data to travel from the indicated source point to the required destination, measured in milliseconds in the last 60 seconds. It helps you evaluate the time required for a packet of data to travel over the network.

You cannot change the granularity of the x-axis to a value that is less than the web granularity you defined in the General tab of the Options dialog box.

Axis | Description
--- | ---
X-axis | Elapsed time since the start of the run.
Y-axis | The average latency—the time in milliseconds required for a packet of data to reach its destination, per 60 second intervals.

When you enable NV for a scenario, you choose the monitoring mode—per group or per load generator. The graph shows the measurements per group or load generator, based on your selection.

If you enabled NV per group, check if a certain group reached a peak during the run compared with other groups whose latency remained constant. This comparison can help you determine which group experienced network issues.

If you enabled NV per load generator and not per group, the graph shows the measurements per load generator.

### See also

- NV monitoring

- Average Bandwidth Utilization monitor graph

- Packet Loss monitor graph

- Total Throughput monitor graph

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 26.1-26.3 All View Local Help Center View Online Help Center Version: