Share this page

# Install NV using the Setup wizard

Install NV using the Setup wizard. You can run the Setup wizard as part of component installation, or as a separate process.

To install NV using the Setup wizard:

1. Run the relevant installation file to open the wizard. For details, see NV installation files.

2. Select an installation mode.

   - Typical: Installs with default options.

   - Custom: Enables you to configure the following options before installation. Some options are enabled only when running the first NV installation on a machine.

     Option | Details
     --- | ---
     Destination Folder | Location of the NV program files. Default: C:\Program Files\OpenText\NV
     Data Folder | Storage location for temporary internal application data and user data, such as test run results. Default: C:\ProgramData\OpenText\NV
     Server Port | NV for Load Generator and VuGen: The port that is used to retrieve NV statistics. NV for Controller: The port that is used for internal NV communication on the machine. Default: 8182
     Enable Remote Connections | Adds an exception to Windows Firewall. Required for NV for Load Generator.

3. Follow the rest of the on-screen instructions to complete the installation.

### See also

- Install Network Virtualization
- Prepare for installation

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 26.1-26.3 All View Local Help Center View Online Help Center Version: