Share this page

# Total Throughput graph

Displays the total data traffic passing to or from the virtualized location( input and output traffic for both the server and client machines), measured in bytes. It helps you evaluate the total amount of load that Vusers generate while running a scenario with NV. You can use this graph to determine where the highest throughput level occurred for a specific group or region.

The legend beneath the graph indicates the line color for each of the metrics.

You cannot change the granularity of the x-axis to a value that is less than the web granularity you defined in the General tab of the Options dialog box.

If you enabled Network Virtualization per load generator (and not per group), the graph shows the measurements per load generator, as shown in the Packet Loss graph.

The following procedure only applies to Analysis, but not to monitoring graphs:

To view information for a specific location:

1. Click within the graph.
2. Select Set Filter/ Sort By from the right-click menu to open the Graph Settings dialog box.
3. In the Filter condition section, select the Location Name row, and select the relevant location from the drop-down list.

Axis | Description
--- | ---
X-axis | Elapsed time since the start of the run.
Y-axis | Throughput of the server, in bytes per second.

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 26.1-26.3 All View Local Help Center View Online Help Center Version: