Share this page

# Known issues for NV

This section describes troubleshooting and limitations for running Vusers with NV.

- The bandwidth utilization measurement is represented in the graphs only when the bandwidth is configured as Shared Bandwidth. If the bandwidth is configured as Individual Bandwidth, bandwidth utilization data does not appear.

- If you upgraded from a version with no NV installed, to the current version with NV installed and enabled, the virtual locations needed to work with NV are not shown. You can manually import the virtual locations.

  Note: When you import virtual locations, you modify the .lrs file. Make a backup of the file if you want to keep the original.

  To import the virtual locations:

  1. In the Controller toolbar, click the Show Virtual Locations Settings button .

  2. In the Virtual Locations Settings dialog box, select the Enable Network Virtualization checkbox, choose Per Group, and click OK.

  3. In the Virtual Location column, where it says none for the virtual location, open the dropdown list and click Browse. A window without locations opens.

  4. Click Import.

  5. Browse to <installdir>Network Virtualization\DefaultLocations\ and select DefaultLocations.xml.

  6. You can now see the virtual locations, and can apply them to the scenario.

- For very large tests, the report generation time may be slow.

- If the NV service is restarted during a scenario run, the network virtualization may fail. Check the service and restart the scenario run.
- Monitoring over a firewall is not supported for scenarios with NV.

- If WinInet replay is enabled in the runtime settings for a web Vuser (Replay > Runtime Settings > Internet Protocol > Preferences > Advanced), you must run the Vuser in per Load Generator mode when using NV—running in per Group mode causes the script to fail.

- NV integration does not comply with all of the accepted Internationalization (I18N) conventions.
- The NV software may consume large amounts of memory, since the technology delays traffic and captures traffic for later analysis. To verify that the load generator machine has sufficient memory, compare the load generator memory consumption with and without the virtualization.

- When running scenarios with virtual locations, Vusers must communicate with the application servers over IPv4. NV emulation is not supported for IPv6 network traffic.

- You cannot run a scenario on the same load generator from two different Controller machines, if they both have NV enabled.
- Location names cannot contain non-English characters.
- NV is not supported with IP Spoofing.

- A scenario is limited to 100 NV emulation flows per load generator. If a scenario is configured with more than 100 flows per load generator, the test will fail. For more information, see this knowledge base article: Network Virtualization: The license for this feature has a limit of 100 flows

  Resolution: Add load generators as needed, so that there are not more that 100 flows on each load generator.

- Running a load or performance test with NV enabled fails with the message "Failed to set NV secret token".

  Cause: The NV secret token fails to update the encoded password in the configuration file during deployment. This behavior is usually caused when cloning machines (or VMs) with NV for Load Generator installed.

  Solution: Recreate a new token after deploying an instance from the source images.

  1. Open the command line as administrator.

  2. Run NV for Load Generator and VuGen setup with template flag on source image. For example:

     NV4LGSetup.exe /v"TEMPLATE=TRUE"

  3. After the installation has finished and you have customized your source image, shut down the machine, but do not reboot (select "No, I will restart my computer later").

  4. Deploy an instance from your image. A Task Scheduler runs (even with a non-admin user), and recreates a new secret token based on your machine ID.

     A log is created under the folder C:\Program Files\OpenText\NV\lib

  For more details, see Software Self-solve knowledge base article KM02889919.

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 26.1-26.3 All View Local Help Center View Online Help Center Version: