Share this page

# MI Listener Configuration dialog box

This dialog box enables you to configure the MI Listener.

Item | Description
--- | ---
To access | Use one of the following methods: Launch the MI Listener Configuration from the OpenText group in the Windows Start menu. Run<installdir>\launch_service\bin\MILsnConfig.exe.
Important information | Before configuring the MI Listener: Open incoming HTTPS service for port 443. The port settings are set by your system administrator. Stop the OpenText Professional Performance Engineering Agent on the MI Listener machine by right-clicking it's icon in the system tray and selecting Close from the popup menu. After configuring the MI Listener: Restart the agent by double-clicking the shortcut on the desktop, or by selecting OpenText Professional Performance Engineering Agent Service in the Windows Start menu. Make sure that no web servers are running on the MI Listener or Monitor-Over-Firewall machine. These servers use port 443 and do not allow the access required by the listening and monitoring processes.
Relevant tasks | Set up an over-firewall deployment

User interface elements are described below:

UI Element | Description
--- | ---
Check Client Certificates | Select True to request that the client send a TLS (SSL) certificate when connecting, and to authenticate the certificate. The default value is False.
Private Key Password | The password that may be required during the certificate authentication process. There is no default value.

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 26.1-26.3 All View Local Help Center View Online Help Center Version: