Share this page

# Total Throughput monitor graph

Displays the total data traffic passing to or from the virtualized location (input and output traffic for both the server and client machines), measured in kilobytes. It helps you evaluate the total amount of load that Vusers generate while running a scenario with NV. The legend below the graph indicates the line color for each of these metrics.

You cannot change the granularity of the x-axis to a value that is less than the web granularity you defined in the General tab of the Options dialog box.

Axis | Description
--- | ---
X-axis | Elapsed time since the start of the run.
Y-axis | Throughput of the server, in kilobytes per second (kBps).

For Analysis (not applicable to monitoring graphs):

To view information for a specific location:

1. Click within the graph.
2. Select Set Filter/ Sort By from the right-click menu to open the Graph Settings dialog box.
3. In the Filter condition section, select the Location Name row, and select the relevant location from the drop-down list.

When you enable Network Virtualization for a scenario, you can choose the monitoring mode—per group or per load generator. The graph shows the measurements per group or load generator, based on your selection.

If you enabled Network Virtualization per group, check which groups experienced low or high throughput. This comparison can help you determine which region experienced network issues.

If you enabled Network Virtualization per load generator, and not per group, the graph shows the throughput for each load generator.

### See also

- NV monitoring

- Average Throughput monitor graph

- Average Latency monitor graph

- Packet Loss monitor graph

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 26.1-26.3 All View Local Help Center View Online Help Center Version: