Share this page

# Infrastructure Resources monitoring

Using the Network Client monitor, you can monitor network client resources for FTP, POP3, SMTP, IMAP, and DNS Vusers during a scenario run and isolate client performance bottlenecks.

The Network Client online monitor graph is only available during scenarios that run relevant scripts, such as FTP or POP3.

You can view this graph by dragging it from the Infrastructure Resources Graph section in the graph tree into the right pane of the Run view. The graph appears in the graph view area.

Network Client performance counters

The following table describes the Network Client measurements that are monitored:

Measurement | Description
--- | ---
Pings per sec | Number of pings per second
Data transfer bytes per sec | Number of data bytes transferred per second
Data receive bytes per sec | Number of data bytes received per second
Connections per sec | Number of connections per second
Accept connections per sec | Number of connections accepted per seconds
SSL Connections per sec | Number of SSL connections per second
SSL Data transfer bytes per sec | Number of SSL data bytes transferred per second
SSL Data receive bytes per sec | Number of SSL data bytes received per second
SSL Accept connections per sec | Number of SSL connections accepted per seconds

Back to top

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 26.1 All View Local Help Center View Online Help Center Version: