# Add / Update AUT Host Dialog Box

This dialog box enables you to add or modify an AUT host.

To access:

- To add an AUT Host: From the LoadRunner Enterprise navigation toolbar, click and select Topologies (under Assets). Click Design Topology. Click AUT Hosts. Click Add New AUT Host .
- To edit topology details: From the LoadRunner Enterprise navigation toolbar, click and select Topologies (under Assets). Click Design Topology. Click AUT Hosts. Select an AUT host and click Update AUT Host .

Note: When creating an AUT host in LoadRunner Enterprise, the AUT host is automatically added to the AUT Pool of the project.

User interface:

User interface elements are described below:

UI Elements | Description
--- | ---
Machine Name/IP | The name or IP of the AUT host machine.
Logical Name | The logical name given to the AUT host.
Platform | The base operating system of the AUT host machine: Window or UNIX.
Protocols | The network protocol used for communication with the AUT host (for monitoring purposes). Default value: NetBIOS, WMI, SSH.
User | The user name for logging in to the AUT host machine.
Password | The password for logging in to the AUT host machine.

Back to top

See also:

- Topologies overview
- Design a topology

https://admhelp.microfocus.com LoadRunner Enterprise 8942
Tips to improve your search results... LoadRunner Enterprise Help Center LoadRunner Enterprise Help LR Enterprise Help 2020_SP2-SP3 All View Local Help Center View Online Help Center back Go back in browser history forward Go forward in browser history Remove search highlights next topic Go to next topic previous topic Go to previous topic Print the current topic Version: