Share this page

# Specify MI Listeners

In Administration, you specify one or more MI Listeners to enable running Vusers or monitoring data over a firewall.

To add an MI Listener:

1. On the Administration sidebar, under Maintenance > Hosts, select MI Listeners.

2. In the MI Listeners tab, click the Add MI Listener button . The New MI Listener page opens.

3. Enter the following details.

   Field | Description
   --- | ---
   MI Listener Name | The host name of the MI Listener. Note: If you have two different IP addresses for the same MI Listener (one for internal communication with the Controller and a second for public communication with a Load Generator located over a firewall), enter the internal IP address here. Enter the public IP address in the Public IP field (see below).
   Description | A description of the MI Listener.
   Public IP | The public IP address of the MI Listener. Note: If you have two different IP addresses for the same MI Listener, one for public communication with a Load Generator located over a firewall and a second for internal communication with the Controller, enter the public IP address here. Enter the internal IP address in the MI Listener Name field (see above).
   Purpose | The role designated to the MI Listener: Monitoring over a firewall Running Vusers over a firewall

4. Click Save. The MI Listener is added to the grid.

https://admhelp.microfocus.com Enterprise Performance Engineering,LoadRunner Enterprise 8942
Tips to improve your search results...OpenText™ Enterprise Performance Engineering Help Center OpenText™ Enterprise Performance Engineering Help 26.1 All View Local Help Center View Online Help Center Version: