Share this page

# vtc_rotate_row

Deprecated. Use lrvtc_rotate_row. Retrieves the first row and moves the values to the bottom.

## C Language

    vtc_rotate_row ( PVCI2 pvci, char **outValues,  unsigned char sendflag );

## C# Language

    bool vts_multi.rotate_row ( long pvci,  string [] outValues, string sendflag );

Query Functions

## Arguments

name | Comments
--- | ---
pvci | The server connection handle.
outValues | Pointer to a string to store retrieved values.
sendflag | Specify how the values are added back to bottom. One of: VTSEND_SAME_ROW - Send all the data to the same row. VTSEND_STACKED - The data is sent to available fields at the bottom of each column. VTSEND_STACKED_UNIQUE - If the value of the first field already exists elsewhere in the column, the top field is retrieved and then discarded. Otherwise, data is sent to an available field at the bottom of the column.

vtc_rotate_row retrieves the data in the first row and stores them in parameters with the same name as the columns. The data is removed from the first row and moved to the bottom of the columns as specified by the unsigned char sendflag.

If there is no data in a cell, the output is `NULL`.

## Return Values

Returns zero on success or one of the Error Codes.

## Parameterization

All string input arguments can be passed using standard parameterization.

## C Language Example

       vtc_rotate_row( pvci, &outColumns, &outValues, VTSEND_STACKED_UNIQUE);
        for(index=0; outColumns[index]; ++index){
            lr_log_message("%s : %s", outColumns[index], outValues[index]);
        }

        vtc_free_list(outColumns);
        vtc_free_list(outValues);

## C# Language Example

.Net Multiple Connection Example

Tips to improve your search results... VuGen Function Reference Version 25.1-25.3 Function Reference 25.1-25.3 All View Local Help Center View Online Help Center Version: