Share this page

# Enhance scripts

This section describes the VuGen features available to enhance Vuser scripts, so that the scripts can accurately generate load. This includes transactions and rendezvous points.

In this topic:

## Add parameterization

When you record a business process, VuGen generates a script that contains the actual values used during recording. If you want to perform the script's actions using different values from those recorded, you replace the recorded values with parameters. This is known as parameterizing the script. For details, see Parameterize scripts.

Back to top

## Insert transactions

You can insert transactions into your Vuser script either while recording the script or after recording the script.

For inserting transactions during recording, use the buttons on the floating toolbar, or click Ctrl +T. For inserting transactions into your script after recording, use the Design > Insert in Script menu items.

For task details, see Using transactions.

Back to top

## Insert rendezvous points

When performing load testing, you may need to emulate heavy user load on your system. To accomplish this, you instruct Vusers to perform a task at exactly the same moment using a rendezvous point. When a Vuser arrives at the rendezvous point, it waits until all Vusers participating in the rendezvous arrive. When the designated number of Vusers arrive, they are released.

You designate the meeting place by inserting a rendezvous point into your Vuser script. When a Vuser executes a script and encounters the rendezvous point, script execution is paused and the Vuser waits for permission from Controller to continue. After the Vuser is released from the rendezvous, it performs the next task in the script.

Note: Rendezvous points are effective only in Action sections—not init or end sections.

You can insert rendezvous points in one of the following ways:

- To insert a rendezvous point while recording, click the Rendezvous button on the Recording toolbar and enter a name in the dialog box (not case sensitive).

- To insert a rendezvous point after recording, select Design > Insert in Script > Rendezvous and enter a name for the rendezvous point (not case sensitive).

When a rendezvous point is inserted, a lr_rendezvous function is added into the Vuser script. For example, the following function defines a rendezvous point named rendezvous1:

    lr_rendezvous("rendezvous1");

Back to top

## Insert steps and functions

You can insert a steps into your script such as think time steps, debug messages, and output messages. For task details, see Steps Toolbox pane.

You insert functions into your script for debugging and to print information about the replay. For a list of some useful functions see VuGen functions.

Back to top

## Insert comments

You can insert comments between Vuser activities. You can insert a comment to describe an activity or to provide information about a specific operation. For example, if you are recording database actions, you could insert a comment to mark the first query, such as "This is the first query."

You can insert a comment in one of the following ways:

- To insert a comment while recording, click the Insert Comment button on the Recording toolbar and enter the comment in the Insert Comment dialog box.

- To insert a comment after recording, select Design > Insert in Script > Comment and enter the comment.

The following script segment shows how a comment appears in a Vuser script:

    /* <comments> */

Back to top

## Insert log messages

You can generate and insert lr_log_message functions into a Vuser script. For example, if you are recording database actions, you could insert a message to indicate the first query, "This is the first query."

To insert a log message, select Design > Insert in Script > Log Message and enter the message.

Back to top

## Insert synchronization points (RTE Vusers only)

You can add synchronization functions to synchronize the execution of the Vuser script with the output from your application. Synchronization applies to RTE Vuser scripts only.

The following is a list of the available synchronization functions:

Function | Description
--- | ---
TE_wait_cursor | Waits for the cursor to appear at a specified location in the terminal window.
TE_wait_silent | Waits for the client application to be silent for a specified number of seconds.
TE_wait_sync | Waits for the system to return from X-SYSTEM or Input Inhibited mode.
TE_wait_text | Waits for a string to appear in a designated location.
TE_wait_sync_transaction | Records the time that the system remained in the most recent X-SYSTEM mode.

For details about synchronization in RTE Vuser scripts, see RTE synchronization overview.

Back to top

See also:

- Replay scripts
- Program Vuser actions
- Use VuGen

https://admhelp.microfocus.com VuGen,Professional Performance Engineering,Performance Engineering for Developers 8942
Tips to improve your search results... OpenText™ Virtual User Generator Help Center OpenText™ VuGen Help 25.1-25.3 All View Local Help Center View Online Help Center Version: