Share this page

# Example: lrs_receive

In the following example, the lrs_receive function connects to Socket 1 and reads the incoming message from buf 2.

    lrs_send("socket1", "buf2", 40, 0);

    lrs_receive("socket1", "buf2", LrsLastArg);

    lrs_close_socket("socket1");

Tips to improve your search results... VuGen Function Reference Version 25.1-25.3 Function Reference 25.1-25.3 All View Local Help Center View Online Help Center Version: