Share this page

# vtc_send_message

Deprecated. User lrvtc_send_message. Sets the last field of a column to a value.

## C Language

    VTCERR2 vtc_send_message ( PVCI2 pvci,  char *columnName, char *value, unsigned short *outRc );

## C# Language

    bool vts_multi.send_message ( long pvci,  string columnName, string value);

Data Update Functions

## Arguments

Name | Comments
--- | ---
pvci | The server connection handle.
columnName | The name of the column.
value | The string to write to the field.
outRc | The status of the operation: 1 - Pass or 0 - Fail

vtc_send_message sets the last field of a column to a value. If there is no empty field in the column, a new row is created.

## Return Values

C Language: Returns zero on success or one of the Error Codes.

C# Language: Returns true on success.

## Parameterization

All string input arguments can be passed using standard parameterization.

## Example

    int colsize, rc;
    char question[30];
        ...
    rc = vtc_column_size(pvci, "O_ID", &colsize);
    ...
    sprintf(question, "order%d_question", colsize);
    rc = vtc_send_message(pvci, "H_question", question, &status);
    lr_log_message("send_if_unique rc=%d\n", rc);

## C# Language Example

.Net Multiple Connection Example

Tips to improve your search results... VuGen Function Reference Version 25.1-25.3 Function Reference 25.1-25.3 All View Local Help Center View Online Help Center Version: