Share this page

# Example: nca_step_end

In the following example, the nca_step_end function indicates the end of the two nca_java_action calls to send to the server as a single packet.

...

    nca_set_window("Note");

    nca_popup_message_press("Note", "OK");

    nca_set_window("Universal Work Queue");

    nca_step_begin();

    nca_java_action("IEU_HGRID_IEU_HGRID_0", "hGridSClick", "P3==String;P2==10011;");

    nca_java_action("IEU_HGRID_IEU_HGRID_0", "hGridSClick", "P3==String;P2==10012;");

    nca_step_end();

    lngTaskCount =0;

    intValidTask =0;

    ...

    Example: Below is the corresponding section of output from the nca_record.log:
    Client Message Properties: action=2 handlerClassId=0x10F handlerId=303
        property=398 type=0xE008 value=Message
        Sub Message Properties: action=2 handlerClassId=0x10F handlerId=303
            property=399 type=0x4000 value="hGridSClick"
            property=400 type=0x4000 value="P3"
            property=401 type=0x4000 value="String"
            property=400 type=0x4000 value="P2"
            property=401 type=0x4000 value="10011"
    Client Message Properties: action=2 handlerClassId=0x10F handlerId=303
        property=398 type=0xE008 value=Message
        Sub Message Properties: action=2 handlerClassId=0x10F handlerId=303
            property=399 type=0x4000 value="hGridSClick"
            property=400 type=0x4000 value="P3"
            property=401 type=0x4000 value="String"
            property=400 type=0x4000 value="P2"
            property=401 type=0x4000 value="10012"

    ...

Tips to improve your search results... VuGen Function Reference Version 25.1-25.3 Function Reference 25.1-25.3 All View Local Help Center View Online Help Center Version: