Share this page

# Example: TE_setvar

In the following example, the script waits for the AUT to stabilize for 5.05 seconds after TE_wait_text, before continuing script execution.

    TE_setvar( TE_SILENT_SEC, 5);

    TE_setvar( TE_SILENT_MILLI, 50);

    TE_wait_text( "Enter secret code:", 30, 29, 13, 1, 13, ret_col, ret_row, ret_text);

Tips to improve your search results... VuGen Function Reference Version 25.1-25.3 Function Reference 25.1-25.3 All View Local Help Center View Online Help Center Version: