Share this page

# vtc_rotate_message

Deprecated. Use lrvtc_rotate_message. Retrieves the first field from the specified column and moves the value to the bottom.

## C Language

    vtc_rotate_message ( PVCI2 pvci, char *columnName, char **outValues, unsigned char sendflag );

## C# Language

    bool vts_multi.rotate_message ( long pvci,  string columnName, string outvalue, string sendflag );

Query Functions

## Arguments

name | Comments
--- | ---
pvci | The server connection handle.
columnName | The name of the column.
outValue | Pointer to a string to store retrieved values.
sendflag | Specify how the value is added back to bottom. One of: VTSEND_STACKED - The data is sent to an available field at the bottom of the column. VTSEND_STACKED_UNIQUE - If the value of the first field already exists elsewhere in the column, the top field is retrieved and then discarded. Otherwise, data is sent to an available field at the bottom of the column.

vtc_rotate_message retrieves the data in the first field of the column and stores it in a parameter with the same name as the column. The data is removed from the first field and moved to the bottom of the column as specified by the unsigned char sendflag.

If there is no data in a cell, the output is `NULL`.

## Return Values

Returns zero on success or one of the Error Codes.

## Parameterization

All string input arguments can be passed using standard parameterization.

## C Language Example

Copy code

        vtc_rotate_message(pvci, "Country", &outValue, VTSEND_STACKED);
        lr_log_message("%s", outValue);
        vtc_free(outValue);

## C# Language Example

.NET Multiple Connection Example

Tips to improve your search results... VuGen Function Reference Version 26.1-26.3 Function Reference 26.1-26.3 All View Local Help Center View Online Help Center Version: