Share this page

# mqtt_await_messages

Waits until there is at least one message in the inbox.

## C Language

size_t mqtt_await_messages( MQTT handle, int timeoutMsec);

MQTT Vuser Functions

## Arguments

Name | Comments
--- | ---
handle | The MQTT client handle returned by mqtt_create.
timeoutMsec | Number of milliseconds or MQTT_DEFAULT. Default: The timeout value in the runtime settings.

## General

mqtt_await_messages waits until there is at least one message in the inbox. The script run continues after there is a message or after the wait times out.

If invalid arguments are passed, the Vuser aborts, even if Continue on error is set.

## Return Values

The number of messages in the inbox. 0 if timed out.

## Parameterization

Standard parameterization is not available for this function.

## Example

// wait for messages to arrive and print the message count

size_t messageCount = mqtt_await_messages(client, MQTT_DEFAULT);

lr_message("There are %d pending messages", messageCount);

if (messageCount > 0) {

// handle messages

}

Tips to improve your search results... VuGen Function Reference Version 26.1-26.3 Function Reference 26.1-26.3 All View Local Help Center View Online Help Center Version: