Share this page

# Perform load testing with nCipher HSM

This task describes how to set up a script to load test an environment with an nCipher HSM (Hardware Security Module).

1. Prerequisite: Generate the client certificate file (client_cert.pem) with the private key (client_key.pem) pointing to the private keys stored in the HSM. Make sure that you can connect to your web server (A.com) with a generated CA file (ca-certs.pem). The successful openssl command should have the following form:

   openssl s_client –connect A.com:443 –CAfile ca-certs.pem –cert client_cert.pem –certform PEM –key client_key.pem – keyform PEM –engine CHIL

2. Set up the PATH environment variable:

   1. Add the nfhwcrhk.dll file, usually located in C:\Program Files (x86)\nCipher\nfast\toolkits\hwcrhk, to the PATH environment variable.
   2. Restart VuGen to apply the changes.

3. Enable nCipher key retrieval

   1. In the runtime settings, go to the Internet Protocol > Preferences view and expand the Authentication section.
   2. Select the Enable retrieving keys from nCipher HSM option. For details, see Preferences View - Internet Protocol.

4. Edit the Vuser script

   Add the following content to the vuser_init section of your Vuser script.

   web_set_sockets_option(SSL_VERSION, "TLS");

   web_set_sockets_option(DEFAULT_VERIFY_PATH, <full_path>\ca-certs.pem);

   web_set_certificate_ex (

   "CertFilePath=<full_path_to_client_cert_file>/client_cert.pem",

   "CertFormat=PEM",

   "KeyFilePath= <full_path_to_client_private_key_file> /client_key.pem",

   "KeyFormat=PEM",

   LAST);

https://admhelp.microfocus.com VuGen,Professional Performance Engineering,Performance Engineering for Developers 8942
Tips to improve your search results... OpenText™ Virtual User Generator Help Center OpenText™ VuGen Help 26.1-26.3 All View Local Help Center View Online Help Center Version: