Share this page

# MQTT Vuser Functions

MQTT (MQ Telemetry Transport) is a publish/subscribe-based messaging protocol for use over the TCP/IP protocol. The protocol is optimized for small bandwidth or unstable networks. It is most commonly used for device-to-device communication as in the Internet of things (IoT).

## Alphabetical List of Functions

Function name | Description
--- | ---
mqtt_await_messages | Waits until there is at least one message in the inbox.
mqtt_clear_inbox | Discards all messages in the inbox.
mqtt_connect | Establishes connection.
mqtt_create | Creates a new connection and returns its handle.
mqtt_disconnect | Disconnects the client from the server.
mqtt_free_message | Releases memory where message is stored.
mqtt_get_length | Returns the message payload length.
mqtt_get_payload | Returns the message payload.
mqtt_get_topic | Returns the message topic.
mqtt_publish | Publishes a message.
mqtt_read_inbox | Reads one message from the inbox and removes the message.
mqtt_set_client_id | Sets the MQTT Client ID.
mqtt_set_credentials | Sets the user name and password.
mqtt_set_lwt | Sets the Last Will and Testament message.
mqtt_set_tls_certificate | Sets the TLS private key file, certificate file and the private key password.
mqtt_set_tls_parameters | Sets the TLS version and cipher list.
mqtt_subscribe | Subscribes the client to a topic.
mqtt_unsubscribe | Unsubscribes the client from a topic.

Tips to improve your search results... VuGen Function Reference Version 26.1 Function Reference 26.1 All View Local Help Center View Online Help Center Version: