Share this page

# TE_type

Send Text Functions

Sends a string to the terminal emulator.

    int TE_type( const char *string );

## Inputs

string | Any string. Special keys are identified using the "<Key>" notation, as described below.

The TE_type function depicts the keyboard input sent to the terminal emulator.

Keyboard input is evaluated to a string using the following conventions:

- Plain text can be input as a regular text string (including blank spaces). For example:

      TE_type("hello, world");

- Input key names longer than one character are represented by identifiers beginning with the letter k, and are bracketed within greater/less than signs (< >). For example, the line:

      TE_type("<kReturn><kControl-y>");

  depicts the input of the Return key followed by the left Control and y keys.

  See TE_type Key Definitions.

- Pauses between keystrokes are indicated by the letter t followed by an integer, representing the number of time units, enclosed by (< >). The statement

  `TE_type("hello, <t3>world");`

  depicts a pause of 3 seconds between the input of the words hello and world. The lowercase t can be replaced by a capital T, which indicates milliseconds.

- Key sequences, in which more than one key is pressed simultaneously, are represented by the sequence of characters, separated by hyphens (-), and enclosed by (< >). The statement

  `TE_type("<kControl-kAlt-kDelete>");`

  Control, Alt, and Delete should be input, and released, simultaneously.

The following characters must be included in angle-brackets when they appear in a TE_type statement:

\ | backslash | <kBackslash>
" | quotes | <kQuote>
> | greater than (only when it appears inside a (< >) clause) | <kGreater>
< | less than (only when it does not appear inside a (<>) clause) | <kLess>

If a script attempts to submit a TE_type statement while the system is in X-SYSTEM mode, the script will wait until the X-SYSTEM mode ends before typing. If the system stays in X-SYSTEM mode for more than TE_XSYSTEM_TIMEOUT milliseconds, then the TE_type function returns a TE_TIMEOUT error. You can set the value of TE_XSYSTEM_TIMEOUT by using TE_setvar. The default value for TE_XSYSTEM_TIMEOUT is 30 seconds.

## Return Values

This function returns 0 if it succeeds, and a negative error code if it fails. It also sets the global variable TE_errno.

## Parameterization

You cannot use standard parameterization for any arguments in this function.

## Example

The following segment sends an amount to be deposited and waits for the client application to respond.

     /* Declare variables for TE_wait_text */

    int ret_row;

    int ret_col;

    char ret_text [80];

    lr_start_transaction (command);

     /* send amount */

    TE_type ("{deposit_amount}<kReturn>");

     /* Wait for response */

    TE_wait_text ("!Operation failed|Withdraw", 30, 1, 1, 0, 0, NULL, NULL, match);

    if (TE_errno != TE_SUCCESS) {

        lr_end_transaction (command, LR_FAIL);

        lr_error_message ("TE_wait_text failed \n);

        return:

    }

    else {

        lr_end_transaction (command, LR_SUCCESS);

    }

Tips to improve your search results... VuGen Function Reference Version 26.1 Function Reference 26.1 All View Local Help Center View Online Help Center Version: