Share this page

# lrvtc_rotate_message

Retrieves the first field from the specified column and moves the value to the bottom.

## C Language

    VTCERR2 lrvtc_rotate_message ( columnName, sendflag );

## C# Language

    void vts.rotate_message ( string columnName,string sendflag  );

## Java Language

int Lrvtc.rotate_message ( String columnName, int sendFlag );

Query Functions

## Arguments

name | Comments
--- | ---
columnName | The name of the column.
sendflag | Specify how the value is added back to bottom. One of: VTSEND_STACKED - The data is sent to an available field at the bottom of the column. VTSEND_STACKED_UNIQUE - If the value of the first field already exists elsewhere in the column, the top field is retrieved and then discarded. Otherwise, data is sent to an available field at the bottom of the column.

lrvtc_rotate_message retrieves the data in the first field of the column and stores it in a parameter with the same name as the column. The data is removed from the first field and moved to the bottom of the column as specified by the sendFlag.

If there is no data in a cell, the output is `NULL`.

## Return Values

C Language: Returns zero on success or one of the Error Codes.

C# Language: No return value.

Java Language: Returns zero on success or one of the Error Codes.

## Parameterization

All string input arguments can be passed using standard parameterization.

## C Language Example

        lrvtc_rotate_message("Country", VTSEND_STACKED);
        lr_log_message(lr_eval_string("{Country}"));

## C# Language Example

.NET Single Connection Example

## Java Language Example

Java Single Connection Example

Tips to improve your search results... VuGen Function Reference Version 26.1 Function Reference 26.1 All View Local Help Center View Online Help Center Version: