Share this page

# Database > Advanced Recording Options dialog box

Enables you set the advanced recording options for database protocols.

Item | Description
--- | ---
To access | Record > Recording Options > Database > Database > Advanced
Important information | This node is available only for specific protocols. For a complete list of protocols and their associated nodes, see Protocol compatibility table.

User interface elements are described below:

UI Element | Description
--- | ---
Recording log options | You can set the detail level for the trace and ASCII log files. Trace file detail level: Off Error Trace. Only logs error messages. Brief Trace. Logs errors and lists the functions generated during recording. Full Trace. Logs all messages, notifications, and warnings. ASCII file detail level: Instructs VuGen to generate ASCII type logs of the recording session. Off Brief detail. Logs all of the functions. Full detail. Logs all of the generated functions and messages in ASCII code.
Code generation buffer size | Specify in kilobytes the maximum size of the code generation buffer. Default value: 128 kilobytes.

Back to top

https://admhelp.microfocus.com VuGen,Professional Performance Engineering,Performance Engineering for Developers 8942
Tips to improve your search results... OpenText™ Virtual User Generator Help Center OpenText™ VuGen Help 26.1 All View Local Help Center View Online Help Center Version: