Share this page

# Passive Mode FTP

In the passive mode FTP protocol, the client initiates both connections to the server. This contrasts with active mode FTP, where the client creates just the initial connection, and then waits to hear from the server on the next port.

Passive mode solves the problem of firewalls filtering out the incoming port connection data from the server.

Tips to improve your search results... VuGen Function Reference Version 26.1 Function Reference 26.1 All View Local Help Center View Online Help Center Version: