Share this page

# Receive and Send Flags

You can specify option flags with the lrs_send and lrs_receive functions:

You can set the following flags options:

Value | Meaning
MSG_PEEK | Peek at the incoming data. The data is copied into the buffer but is not removed from the input queue.(lrs_receive only)
MSG_DONTROUTE | Don't include routing information in the message. This is only meaningful with output operations (lrs_send only), and is usually only used for diagnostic or routing programs.
MSG_OOB | Send or receive out-of-band (OOB) data. OOB data is an independent transmission that can be sent along with each pair of receive-send streams. OOB data may be delivered independently of the regular data, so it does not interrupt the normal stream. It is often used for urgent messages.

Tips to improve your search results... VuGen Function Reference Version 26.1 Function Reference 26.1 All View Local Help Center View Online Help Center Version: