Share this page

# Advanced Port Mapping Settings dialog box

Enables you to set the advanced port mapping settings. For more information, see Port mapping auto detection.

To access: Record > Recording Options > Network > Mapping and Filtering. Click Options in the Port Mapping section.

User interface elements are described below:

UI Element | Description
--- | ---
Enable auto SSL detection | Automatically detects SSL communication. Note that this applies only to port mappings that were defined as auto in the Connection type box, or not defined at all. If a server, port, or server:port combination was defined as either Plain or SSL, then auto SSL detection does not apply. SSL Version: Specify the version that you want to detect. SSL Ciphers: Specify the cipher to detect: To enable OpenSSL to choose the default cipher automatically, select (Default OpenSSL Ciphers) in the dropdown list . To define your own cipher and add it to the dropdown list, select (New SSL Cipher) and type in the cipher string. To remove a user-defined cipher, select the cipher in the list and click the button. For more information on OpenSSL cipher strings, refer to the OpenSSL Cipher documentation.
Enable auto detection of SOCKET based communication | Automatically detects the type of communication. If required, raise the maximum number of transitions, one at a time until VuGen succeeds in detecting the protocol. You can also gradually increase the maximum buffer size by 1024 bytes (1 KB) at a time until VuGen succeeds in detecting the protocol. This allows VuGen to review a larger amount of data in order to find a signature.
Log Level | Sets the logging level for the automatic socket detection.

Back to top

See also:

- Protocol compatibility table

https://admhelp.microfocus.com VuGen,Professional Performance Engineering,Performance Engineering for Developers 8942
Tips to improve your search results... OpenText™ Virtual User Generator Help Center OpenText™ VuGen Help 26.1 All View Local Help Center View Online Help Center Version: