Share this page

# Connect to an enterprise wireless network (Tech preview)

You can use a REST API call to connect a device to a corporate Wi-Fi network. For example, if you have several testing environments, you may need to connect the device to a different network before running an automated test. You may also need to switch to a different network if the network disconnects.

## Before you start - iOS devices

iOS devices require a special entitlement to call the API. Therefore, the Wi-Fi app must be installed on any iOS device you want to connect to a Wi-Fi network using the API.

Limitations

Note the following limitations for the WiFi app:

1. The app is supported only on iOS 13 and later.

2. The app should not be re-signed. It uses an Enterprise certificate that needs to be trusted before the app can be run.

Install the WiFi app

1. Locate the WiFi app. The default location is /opt/FunctionalTestingLabForMobileAndWeb/connector/Agent/WiFi/

2. Install the app by running the command `ideviceinstaller -i <ipaPath>` or upload the app to server and install it on the device using the remote device access window.

3. The app is signed with an Enterprise certificate, therefore you may get an Untrusted Enterprise Developer alert when you first open it. To trust the app, go to Settings > General > VPN & Device Management and click MicroFocus Ltd. In the Trust dialog, click Trust.

4. Open the app. An alert is displayed. If the app attempts to open the Agent app on your device, click Open.

5. Input the necessary network information. Switch on Debug Mode. Click Connect WiFi.

   Caution: Always make sure Debug Mode is switched off when using this app in a production environment.

## Use REST API to set a Wi-Fi network connection on device

Use a REST API call to connect the device to a Wi-Fi network.

The /v2/devices/{deviceId}/jobs/{jobId}/WiFi/{ssid} method attempts to establish a connection to the given Wi-Fi network. If the connection is successful, the device connects to the specified network.

Follow these guidelines for the WiFi details.

Parameter | Details
--- | ---
enterpriseType | The Extensible Authentication Protocol type used. iOS: EAPTLS; EAPTTLS; EAPPEAP; EAPFAST. Generally, the value is EAPPEAP. Android: PEAP; TLS; TTLS; PWD; SIM; AKA; WFA-UNAUTH-TLS;WAPI_CERT
enterpriseName | Your username for the enterprise Wi-Fi network
enterprisePassphrase | Your password for the enterprise Wi-Fi network.
enterpriseDomain | The server name for the enterprise Wi-Fi network.

For details on the required parameters and response body, see the Devices PUT section in the REST API reference. For more details, see REST API reference.

https://admhelp.microfocus.com/Functional Testing Lab 8942
Tips to improve your search results... OpenText™ Functional Testing Lab for Mobile and Web Help Center OpenText™ Functional Testing Lab Help 25.2 All View Local Help Center View Online Help Center Version: