Share this page

# UNIX Resources Default Measurements

The following default measurements are available for UNIX machines:

Measurement | Description
--- | ---
Average load | Average number of processes simultaneously in `Ready' state during the last minute.
Collision rate | Collisions per second detected on the Ethernet.
Context switches rate | Number of switches between processes or threads, per second.
CPU utilization | Percent of time that the CPU is utilized.
Disk rate | Rate of disk transfers.
Incoming packets error rate | Errors per second while receiving Ethernet packets.
Incoming packets rate | Incoming Ethernet packets per second.
Interrupt rate | Number of device interrupts per second.
Outgoing packets errors rate | Errors per second while sending Ethernet packets.
Outgoing packets rate | Outgoing Ethernet packets per second.
Page-in rate | Number of pages read to physical memory, per second.
Page-out rate | Number of pages written to pagefile(s) and removed from physical memory, per second.
Paging rate | Number of pages read to physical memory or written to pagefile(s), per second.
Swap-in rate | The rate by which disk content is swapped into the machine's memory in kBps.
Swap-out rate | The rate by which the machine's memory is being swapped out to disk in kBps.
System mode CPU utilization | Percent of time that the CPU is utilized in system mode.
User mode CPU utilization | Percent of time that the CPU is utilized in user mode.

Back to top

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 25.1-25.3 All View Local Help Center View Online Help Center Version: