Share this page

# Connections per Second graph

This graph shows the number of new TCP/IP connections opened and the number of connections that are shut down for each second of the load test scenario.

Tip: The number of new connections should be a small fraction of the number of hits per second, because new TCP/IP connections use a lot of server, router, and network resources. Ideally, multiple HTTP requests should use the same connection, instead of opening a new connection for each request.

Axis | Description
--- | ---
X-axis | Elapsed time since the start of the run.
Y-axis | TCP/IP connections that were opened.

Back to top

See also:

- Error graphs

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 25.1-25.3 All View Local Help Center View Online Help Center Version: