Share this page

# Network Delay Time graph

This graph shows the delays for the complete path between the source and destination machines (for example, the database server and Vuser load generator). The graph maps the delay as a function of the elapsed load test scenario time.

For example, you can have a merged graph comparing network delays to running Vusers. If the graph shows a network delay when a large number of Vusers are running, this could indicate an overloaded network.

Each path defined in Controller is represented by a separate line with a different color in the graph.

Item | Description
--- | ---
X-axis | Elapsed time since the start of the run.
Y-axis | Network delay time.
Tips | You can merge various graphs to determine if the network is a bottleneck. For example, using the Network Delay Time and Running Vusers graphs, you can determine how the number of Vusers affects the network delay.

Back to top

See also:

- Network delay monitoring
- Network Monitor graphs

https://admhelp.microfocus.com Professional Performance Engineering,VuGen 8942
Tips to improve your search results... OpenText™ Professional Performance Engineering Help Center OpenText™ Professional Performance Engineering Help 25.1-25.3 All View Local Help Center View Online Help Center Version: