Share this page

# Application Server

We recommend the following for PPM Servers:

- Processors equivalent to current generation 2.66-3.00 GHz Intel� Xeon� multi-core processors (dual-core or quad-core).

- Minimum of 2 CPU cores per host to best support multi-threaded nature of PPM

- JVM heap size of 1280 MB. (This is the default.) Under heavy load, a JVM running with a 1280-MB heap consumes upward of 1500 MB, including native area code.

- Provision hardware to support 1.5 GB of RAM for each PPM node in a server cluster.

- If clients access PPM over a wide area network (WAN), enable both dynamic asset compression and keepalive on the external Web server.

https://admhelp.microfocus.com PPM 8942
Tips to improve your search results... OpenText™ Project and Portfolio Management Help Center PPM Help 26.2-26.3 All View Local Help Center View Online Help Center Version: