Share this page

# Solution Configuration 3

Solution Configuration 3, which is shown in the following figure, builds on Solution Configuration 2. This is a mission-critical server cluster configuration that includes clustered application hosts and an external Web tier.

Solution Configuration 3 has the following features:

- Six physical servers:

  - Two for the Web tier

  - Two for the application tier

  - Two for the database tier

- Two external Web servers, which reside on separate hosts

- User traffic distributed across physical hosts and nodes

- Two nodes dedicated to handling PPM services

- Application nodes configured in a server cluster support service failover

- 10 to 12 GB RAM for each application server (recommended)

Solution Configuration 3 is ideal if your project must have the following:

- Continuous application availability with minimized system outages

- Single sign-on support

- Need for future growth

https://admhelp.microfocus.com PPM 8942
Tips to improve your search results... OpenText™ Project and Portfolio Management Help Center PPM Help 26.2-26.3 All View Local Help Center View Online Help Center Version: